**Installation Notes**

CLC Firmware 0.1.27







Prior to installing, it is recommended to review the CLC Firmware 0.1.27 Release Notes. The following are the instruction to install the firmware update.

# Accessing CLC Firmware

The website is the primary means for delivering firmware. If a CD is desired, one can be requested by contacting DSI Customer Service (CService@datasci.com).

1. Navigate to [www.datasci.com](http://www.datasci.com)
2. Browse to **Resources | DSI Gateway Portal**.
3. Login using your **User Name** and **Password**. If you have forgotten or do not have a User Name and Password, the ability to request a new password or register at the site is available.
4. Select **Software Updates**.
5. Click the **CLC 0.1.27.zip** to download the contents to a desired location.
6. Extract the files by **right-clicking** the .zip file and choosing **Extract**.

# Installing CLC Firmware

1. With the CLC connected to the system, launch **Ponemah**.
2. Select **Hardware | PhysioTel Digital Diagnostics…***Note*: If using *Ponemah v5.20*, select **Hardware | Diagnostics…**
3. Choose the CLC from the *Name – Model Name (Serial Number)* dropdown.  
   *Note:* Select the Refresh List button if the CLC does not appear in the dropdown list.  
     
   
4. Select the *Upload CLC Firmware* link from the list view on the left side of diagnostics page.  
     
   
5. **Please complete steps a. – d. below twice.**
   1. Select the **Browse…** button.  
      
   2. Select the *CLC 0.1.27* file obtained during the .zip extract step above. Once uploaded, the following message will appear: *Validated. Upgrade will be applied during reboot.*
   3. Select the **reboot** link within the message to navigate to the *Reboot* diagnostics page.  
        
      
   4. Select the **Reboot** button.  
        
      